| LCD Library 1.3.0 LCD Library - LCD control class hierarchy library. Drop in replacement for the LiquidCrystal Library.

- Main Page
- Classes
- Files

- File List
- File Members

LiquidCrystal_I2C.h
Go to the documentation of this file.

    00001 // ---------------------------------------------------------------------------
    00002 // Created by Francisco Malpartida on 20/08/11.
    00003 // Copyright 2011 - Under creative commons license 3.0:
    00004 //        Attribution-ShareAlike CC BY-SA
    00005 //
    00006 // This software is furnished "as is", without technical support, and with no
    00007 // warranty, express or implied, as to its usefulness for any purpose.
    00008 //
    00009 // Thread Safe: No
    00010 // Extendable: Yes
    00011 //
    00012 // @file LiquidCrystal_I2C.h
    00013 // This file implements a basic liquid crystal library that comes as standard
    00014 // in the Arduino SDK but using an I2C IO extension board.
    00015 //
    00016 // @brief
    00017 // This is a basic implementation of the LiquidCrystal library of the
    00018 // Arduino SDK. The original library has been reworked in such a way that
    00019 // this class implements the all methods to command an LCD based
    00020 // on the Hitachi HD44780 and compatible chipsets using I2C extension
    00021 // backpacks such as the I2CLCDextraIO with the PCF8574* I2C IO Expander ASIC.
    00022 //
    00023 // The functionality provided by this class and its base class is identical
    00024 // to the original functionality of the Arduino LiquidCrystal library.
    00025 //
    00026 //
    00027 // @author F. Malpartida - fmalpartida@gmail.com
    00028 // ---------------------------------------------------------------------------
    00029 #ifndef LiquidCrystal_I2C_h
    00030 #define LiquidCrystal_I2C_h
    00031 #include <inttypes.h>
    00032 #include <Print.h>
    00033
    00034 #include "I2CIO.h"
    00035 #include "LCD.h"
    00036
    00037
    00038 class LiquidCrystal_I2C : public LCD
    00039 {
    00040 public:
    00041
    00051    LiquidCrystal_I2C (uint8_t lcd_Addr);
    00052    // Constructor with backlight control
    00053    LiquidCrystal_I2C (uint8_t lcd_Addr, uint8_t backlighPin, t_backlighPol pol);
    00054
    00067    LiquidCrystal_I2C( uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs);
    00068    // Constructor with backlight control
    00069    LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs,
    00070                      uint8_t backlighPin, t_backlighPol pol);
    00071
    00088    LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs,
    00089                      uint8_t d4, uint8_t d5, uint8_t d6, uint8_t d7 );
    00090    // Constructor with backlight control
    00091    LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs,
    00092                      uint8_t d4, uint8_t d5, uint8_t d6, uint8_t d7,
    00093                      uint8_t backlighPin, t_backlighPol pol);
    00110    virtual void begin(uint8_t cols, uint8_t rows, uint8_t charsize = LCD_5x8DOTS);
    00111
    00124    virtual void send(uint8_t value, uint8_t mode);
    00125
    00134    void setBacklightPin ( uint8_t value, t_backlighPol pol );
    00135
    00145    void setBacklight ( uint8_t value );
    00146
    00147 private:
    00148
    00154    int  init();
    00155
    00171    void config (uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs,
    00172                 uint8_t d4, uint8_t d5, uint8_t d6, uint8_t d7 );
    00173
    00182    void write4bits(uint8_t value, uint8_t mode);
    00183
    00190    void pulseEnable(uint8_t);
    00191
    00192
    00193    uint8_t _Addr;             // I2C Address of the IO expander
    00194    uint8_t _backlightPinMask; // Backlight IO pin mask
    00195    uint8_t _backlightStsMask; // Backlight status mask
    00196    I2CIO   _i2cio;            // I2CIO PCF8574* expansion module driver I2CLCDextraIO
    00197    uint8_t _En;               // LCD expander word for enable pin
    00198    uint8_t _Rw;               // LCD expander word for R/W pin
    00199    uint8_t _Rs;               // LCD expander word for Register Select pin
    00200    uint8_t _data_pins[4];     // LCD data lines
    00201
    00202 };
    00203
    00204 #endif

All Classes Files Functions Variables Typedefs Enumerations Enumerator Defines